|RECORD=BOM|VERSION=2|FILENAME=D:\PRJ\GIT_PRJ\EVU-LI-2.1\evu-li-2.1\EVU-LI-2.1.$$$|KIND=ALTIUM_DESIGNER_LIVEBOM|DATE=20.01.2026|TIME=14:24:34|CURRENCY=USD|PRODUCTIONQUANTITY=1|PERUNITTARGETPRICE=0|PERUNITACTUALPRICE=0
|RECORD=GeneralOptions|OPENEXPORTED=False|ADDTOPROJECT=False|FORCEFIT=False|NOTFITTED=False|TEMPLATEFILENAME=|BATCHMODE=0|SUPPLIERPRODQTY=0|SUPPLIERAUTOQTY=False|SUPPLIERUSECACHEDPRICING=False|SUPPLIERCURRENCY=|SOLUTIONSPERITEM=1|SUPPLIERSPERSOLUTION=1|DISPLAYTOTALROW=False|DISPLAYSUBTOTALSFORGROUPS=False|INCLUDEPCBPARAMETERS=False|INCLUDEDBPARAMETERS=False|INCLUDEVAULTPARAMETERS=False|INCLUDECLOUDPARAMETERS=False|INCLUDEDOCUMENTPARAMETERS=False|FILTEROUTRISKYSOLUTIONS=True|DESIGNATORGROUPING=No
|RECORD=SortOrderOptions|SORTORDER=
|RECORD=GroupOrderOptions|GROUPORDER=
|RECORD=VisibleOrderOptions|VISIBLEORDER=Line #=58!Designator=163!Comment=182!Quantity=71!Description=208!Manufacturer=148!Note=50!DNP=41
|RECORD=VisibleOrderOptions2|BASEVIEW=Line #=58!Designator=163!Comment=182!Quantity=71!Description=208!Manufacturer=148!Note=50!DNP=41|FLATVIEW=Line #=54!Comment=-1!Description=-1!Designator=80!Manufacturer 1=102!Manufacturer Part Number 1=169!Manufacturer Lifecycle 1=147!Supplier 1=75!Supplier Part Number 1=142!Supplier Unit Price 1=127!Supplier Subtotal 1=122|CONSOLIDATEDVIEW=Line #=54!Comment=-1!Description=-1!Designator=-1!Quantity=67!Manufacturer 1=102!Manufacturer Part Number 1=169!Manufacturer Lifecycle 1=147!Supplier 1=75!Supplier Part Number 1=142!Supplier Unit Price 1=127!Supplier Subtotal 1=122!Quantity@EVU-LI-2.1=102!Price@EVU-LI-2.1=109
|RECORD=CustomColumns|CUSTOMCOLUMNS=
|RECORD=ColumnsAliases|COLUMNSALIASES=Comment=Name!Quantity@EVU-LI-2.1=EVU-LI-2.1 - Qty!Price@EVU-LI-2.1=EVU-LI-2.1 - Price
|RECORD=FilterOptions|FILTER=
|RECORD=CheckGroupCompParamsOptions|CHECKGROUPCOMPPARAMS=Comment=0,Description=0,Value=0,Footprint=1
|RECORD=ManufacturerLinkOptions|MANUFACTURERLINKPARAMETERS=
|RECORD=FavoriteSuppliers|PARTSOURCES=|SUPPLIERS=|USESUPPLIERORDER=False
|RECORD=CheckOptions|CHECKLEVELS=
|RECORD=LineNumberingOptions|STARTVALUE=|INCREMENT=
|RECORD=Catalog|DBLINKFILEPATH=
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=EVU-LI-2.0.SCHLIB\GRM155R71C104KA88D|DESIGNITEMID=GRM155R71C104KA88D|ITEMSOURCE=EVU-LI-2.0.SCHLIB|STATUS=Unknown|DESCRIPTION=0402 X7R  0,1 uF±10% 16V|USERCOMMENTS=GRM155R71C104KA88D|NOTE=|LINENUMBER=|SELECTEDPARAMETERSHASH="0402 X7R  0,1 uF±10% 16V",100nF,GRM155R71C104KA88D|COMPONENTPARAMETERS=Comment=GRM155R71C104KA88D,"Component Kind=Standard",ComponentHeight=0.5mm,ComponentLink1Description=DataSheet,"ComponentLink1URL=\\STORAGE\Lib_PCAD\LIB_DataSheet\Capacitors\Murata Chip Monolithic Ceramic Capacitors.pdf","Description=0402 X7R  0,1 uF±10% 16V",Footprint=CAPC1005X50N,"Ibis Model=","Library Name=EVU-LI-2.0.SCHLIB","Library Reference=GRM155R71C104KA88D","Manufacturer=""Murata""",ManufacturerPartNumber=GRM155R71C104KA88D,"NOM=0402 X7R 100nF ±10% 16Â",PCB3D=,"Pin Info=",Power_Voltage=16Â,"Signal Integrity=",Simulation=,"TKE=0402 X7R",Tolerance=±10%,Value=100nF,"Value Ru=0,1 ìêÔ",Ïðèìå÷àíèå=|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=EVU-LI-2.1.SCHLIB\GRM155R71C104KA88D|DESIGNITEMID=GRM155R71C104KA88D|ITEMSOURCE=EVU-LI-2.1.SCHLIB|STATUS=Unknown|DESCRIPTION=0402 X7R  0,1 uF±10% 16V|USERCOMMENTS=GRM155R71C104KA88D|NOTE=|LINENUMBER=|SELECTEDPARAMETERSHASH="0402 X7R  0,1 uF±10% 16V",100nF,GRM155R71C104KA88D|COMPONENTPARAMETERS=Comment=GRM155R71C104KA88D,"Component Kind=Standard",ComponentHeight=0.5mm,ComponentLink1Description=DataSheet,"ComponentLink1URL=\\STORAGE\Lib_PCAD\LIB_DataSheet\Capacitors\Murata Chip Monolithic Ceramic Capacitors.pdf","Description=0402 X7R  0,1 uF±10% 16V",Footprint=CAPC1005X50N,"Ibis Model=","Library Name=EVU-LI-2.1.SCHLIB","Library Reference=GRM155R71C104KA88D","Manufacturer=""Murata""",ManufacturerPartNumber=GRM155R71C104KA88D,"NOM=0402 X7R 100nF ±10% 16Â",PCB3D=,"Pin Info=",Power_Voltage=16Â,"Signal Integrity=",Simulation=,"TKE=0402 X7R",Tolerance=±10%,Value=100nF,"Value Ru=0,1 ìêÔ",Ïðèìå÷àíèå=|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=EVU-LI-2.1.SCHLIB\BE-U1000|DESIGNITEMID=BE-U1000|ITEMSOURCE=EVU-LI-2.1.SCHLIB|STATUS=Unknown|DESCRIPTION=Microcontroller BE-U1000|USERCOMMENTS=BE-U1000|NOTE=|LINENUMBER=|SELECTEDPARAMETERSHASH=,BE-U1000,"Microcontroller BE-U1000"|COMPONENTPARAMETERS=Availability=,Comment=BE-U1000,"Component Kind=Standard","Description=Microcontroller BE-U1000",Footprint=QFNWB10X10-88L-AL,"Ibis Model=","Library Name=EVU-LI-2.1.SCHLIB","Library Reference=BE-U1000","Manufacturer=""Baikal Electronics""",MF=,MP=,Package=None,PCB3D=,"Pin Info=",Price=None,"Signal Integrity=",Simulation=,"TKE=QFN 88",Value=|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=EVU-LI-2.0.SCHLIB\MT25QL128ABA1EW7-0SIT|DESIGNITEMID=MT25QL128ABA1EW7-0SIT|ITEMSOURCE=EVU-LI-2.0.SCHLIB|STATUS=Unknown|DESCRIPTION=FLASH 128MBIT SPI 8WPDFN|USERCOMMENTS=MT25QL128ABA1EW7-0SIT|NOTE=|LINENUMBER=|SELECTEDPARAMETERSHASH="FLASH 128MBIT SPI 8WPDFN",MT25QL128ABA1EW7-0SIT|COMPONENTPARAMETERS="Arrow Part Number=MT25QL128ABA1ESE-0SIT TR","Arrow Price/Stock=https://www.arrow.com/en/products/mt25ql128aba1ese-0sittr/micron-technology?region=nac",Comment=MT25QL128ABA1EW7-0SIT,"Component Kind=Standard","Datasheet Link=https://datasheet.datasheetarchive.com/originals/distributors/DKDS42/DSANUWW0045431.pdf","Description=FLASH 128MBIT SPI 8WPDFN",Footprint=W-PDFN-8(5x6),Height=2.16mm,"Ibis Model=","Library Name=EVU-LI-2.0.SCHLIB","Library Reference=MT25QL128ABA1EW7-0SIT","Manufacturer=""Micron""",Manufacturer_Part_Number=MT25QL128ABA1EW7-0SIT,"Mouser Part Number=340-224871-REEL","Mouser Price/Stock=https://www.mouser.co.uk/ProductDetail/Micron/MT25QL128ABA1ESE-0SIT-TR?qs=j%252B1pi9TdxUbjYudTgg%2Fegw%3D%3D",PCB3D=,"Pin Info=","Signal Integrity=",Simulation=|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=EVU-LI-2.1.SCHLIB\AP2112K-3.3TRG1|DESIGNITEMID=AP2112K-3.3TRG1|ITEMSOURCE=EVU-LI-2.1.SCHLIB|STATUS=Unknown|DESCRIPTION=LDO voltage regulator|USERCOMMENTS=AP2112K-3.3TRG1|NOTE=|LINENUMBER=|SELECTEDPARAMETERSHASH=AP2112K-3.3TRG1,"LDO voltage regulator"|COMPONENTPARAMETERS="Arrow Part Number=AP2112K-3.3TRG1","Arrow Price/Stock=https://www.arrow.com/en/products/ap2112k-3.3trg1/diodes-incorporated?utm_currency=USD&region=europe",Comment=AP2112K-3.3TRG1,"Component Kind=Standard","Datasheet Link=https://www.diodes.com//assets/Datasheets/AP2112.pdf","Description=LDO voltage regulator",Footprint=SOT95P285X140-5N,Height=1.4mm,"Ibis Model=","Library Name=EVU-LI-2.1.SCHLIB","Library Reference=AP2112K-3.3TRG1","Manufacturer=""Diodes""","Manufacturer_Name=Diodes Incorporated",Manufacturer_Part_Number=AP2112K-3.3TRG1,"Mouser Part Number=621-AP2112K-3.3TRG1","Mouser Price/Stock=https://www.mouser.co.uk/ProductDetail/Diodes-Incorporated/AP2112K-3.3TRG1?qs=x6A8l6qLYDDPYHosCdzh%2FA%3D%3D",PCB3D=,"Pin Info=","Signal Integrity=",Simulation=|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=EVU-LI-2.0.SCHLIB\USBLC6-2SC6|DESIGNITEMID=USBLC6-2SC6|ITEMSOURCE=EVU-LI-2.0.SCHLIB|STATUS=Unknown|DESCRIPTION=Very low capacitance ESD protector|USERCOMMENTS=USBLC6-2SC6|NOTE=|LINENUMBER=|SELECTEDPARAMETERSHASH=,USBLC6-2SC6,"Very low capacitance ESD protector"|COMPONENTPARAMETERS=Comment=USBLC6-2SC6,"Component Kind=Standard",ComponentHeight=1.45mm,ComponentLink1Description=DataSheet,ComponentLink1URL=\\STORAGE\Lib_PCAD\LIB_DataSheet\IC\STMicroelectronics\USBLC6-2SC6.pdf,"Description=Very low capacitance ESD protector",Footprint=SOT95P280X145-6N,"Ibis Model=","Library Name=EVU-LI-2.0.SCHLIB","Library Reference=USBLC6-2SC6","Manufacturer=""STMicroelectronics""",ManufacturerPartNumber=USBLC6-2SC6,MARK=UL26,"NOM=  ",PCB3D=,"Pin Info=",Power_Voltage=,"Signal Integrity=",Simulation=,TKE=,Tolerance=,Value=,Ïðèìå÷àíèå=|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=EVU-LI-2.0.SCHLIB\JFC0603-0500FS|DESIGNITEMID=JFC0603-0500FS|ITEMSOURCE=EVU-LI-2.0.SCHLIB|STATUS=Unknown|DESCRIPTION=Fuse 500mA 32V 0603|USERCOMMENTS=JFC0603-0500FS|NOTE=|LINENUMBER=|SELECTEDPARAMETERSHASH=500mA,"Fuse 500mA 32V 0603",JFC0603-0500FS|COMPONENTPARAMETERS=Comment=JFC0603-0500FS,"Component Kind=Standard",ComponentHeight=0.48mm,ComponentLink1Description=DataSheet,"ComponentLink1URL=\\STORAGE\Lib_PCAD\LIB_DataSheet\PROTECTORS\LITTEL FUSE\Littelfuse_Fuse_466.pdf","Description=Fuse 500mA 32V 0603",Footprint=RESC1608X45N,"Ibis Model=","Library Name=EVU-LI-2.0.SCHLIB","Library Reference=JFC0603-0500FS","Manufacturer=""JDT Fuse Industrial""",ManufacturerPartNumber=JFC0603-0500FS,MARK=F,"NOM= 500mA ",PCB3D=,"Pin Info=",Power_Voltage=,"Signal Integrity=",Simulation=,TKE=,Tolerance=,Value=500mA,Ïðèìå÷àíèå=|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=EVU-LI-2.0.SCHLIB\OT252025MJBA4SL|DESIGNITEMID=OT252025MJBA4SL|ITEMSOURCE=EVU-LI-2.0.SCHLIB|STATUS=Unknown|DESCRIPTION=3.3V ±10ppm 5mA ±20ppm CMOS 25MHz  Oscillator|USERCOMMENTS=OT252025MJBA4SL|NOTE=|LINENUMBER=|SELECTEDPARAMETERSHASH="3.3V ±10ppm 5mA ±20ppm CMOS 25MHz  Oscillator",OT252025MJBA4SL|COMPONENTPARAMETERS="Arrow Part Number=","Arrow Price/Stock=",Comment=OT252025MJBA4SL,"Component Kind=Standard","Datasheet Link=https://wmsc.lcsc.com/wmsc/upload/file/pdf/v2/lcsc/2304140030_YXC-OT322525MJBA4SL_C669088.pdf","Description=3.3V ±10ppm 5mA ±20ppm CMOS 25MHz  Oscillator",Footprint=Crystal_4-SMD_2.5x2.0,Height=1mm,"Ibis Model=","Library Name=EVU-LI-2.0.SCHLIB","Library Reference=OT252025MJBA4SL","Manufacturer=""YXC""",Manufacturer_Part_Number=OT322525MJBA4SL,"Mouser Part Number=","Mouser Price/Stock=",PCB3D=,"Pin Info=","Signal Integrity=",Simulation=,TKE=SMD3225-4P|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=EVU-LI-2.0.SCHLIB\BLM15AX601SN1|DESIGNITEMID=BLM15AX601SN1|ITEMSOURCE=EVU-LI-2.0.SCHLIB|STATUS=Unknown|DESCRIPTION=600 Ohms/100MHz 0,5A 0,34 Ohms|USERCOMMENTS=BLM15AX601SN1|NOTE=|LINENUMBER=|SELECTEDPARAMETERSHASH="600 Ohms/100MHz 0,5A 0,34 Ohms","600 Îì/100MÃö 0,5A 0,34 Îì",BLM15AX601SN1|COMPONENTPARAMETERS=Comment=BLM15AX601SN1,"Component Kind=Standard",ComponentHeight=0.5mm,ComponentLink1Description=DataSheet,ComponentLink1URL=\\STORAGE\Lib_PCAD\LIB_DataSheet\FILTERS\MURATA\Êàòàëîã_murata.pdf,"Description=600 Ohms/100MHz 0,5A 0,34 Ohms",Footprint=BLM15X10X05X50N,"Ibis Model=","Library Name=EVU-LI-2.0.SCHLIB","Library Reference=BLM15AX601SN1","Manufacturer=""Murata""",ManufacturerPartNumber=BLM15AX601SN1,MARK=,"NOM=600 Îì/100MÃö 0,5A 0,34 Îì",PCB3D=,"Pin Info=",Power_Voltage=,"Signal Integrity=",Simulation=,TKE=,Tolerance=,"Value=600 Îì/100MÃö 0,5A 0,34 Îì",Ïðèìå÷àíèå=|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=EVU-LI-2.0.SCHLIB\KPT-1608PWF-A|DESIGNITEMID=KPT-1608PWF-A|ITEMSOURCE=EVU-LI-2.0.SCHLIB|STATUS=Unknown|DESCRIPTION=0603 LED Diod SMD White|USERCOMMENTS=KPT-1608PWF-A|NOTE=|LINENUMBER=|SELECTEDPARAMETERSHASH=,"0603 LED Diod SMD White",KPT-1608PWF-A|COMPONENTPARAMETERS=Comment=KPT-1608PWF-A,"Component Kind=Standard",ComponentHeight=0.75mm,ComponentLink1Description=DataSheet,ComponentLink1URL=\\STORAGE\Lib_PCAD\LIB_DataSheet\DIODES_LED\KINGBRIGHT\KPT-1608.pdf,"Description=0603 LED Diod SMD White",DNP=,Footprint=KPT1608X16X08X75N_LINE,"Ibis Model=","Library Name=EVU-LI-2.0.SCHLIB","Library Reference=KPT-1608PWF-A","Manufacturer=""Kingbright""",ManufacturerPartNumber=KPT-1608PWF-A,MARK=,NOM=,"Parameter 1=",PCB3D=,"Pin Info=",Power_Voltage=,"Signal Integrity=",Simulation=,TKE=0603,Tolerance=,Value=,Ïðèìå÷àíèå=|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=EVU-LI-2.0.SCHLIB\KPT-1608SGC|DESIGNITEMID=KPT-1608SGC|ITEMSOURCE=EVU-LI-2.0.SCHLIB|STATUS=Unknown|DESCRIPTION=0603 LED Diod SMD Green|USERCOMMENTS=KPT-1608SGC|NOTE=|LINENUMBER=|SELECTEDPARAMETERSHASH=,"0603 LED Diod SMD Green",KPT-1608SGC|COMPONENTPARAMETERS=Comment=KPT-1608SGC,"Component Kind=Standard",ComponentHeight=0.75mm,ComponentLink1Description=DataSheet,ComponentLink1URL=\\STORAGE\Lib_PCAD\LIB_DataSheet\DIODES_LED\KINGBRIGHT\KPT-1608.pdf,"Description=0603 LED Diod SMD Green",DNP=,Footprint=KPT1608X16X08X75N_LINE,"Ibis Model=","Library Name=EVU-LI-2.0.SCHLIB","Library Reference=KPT-1608SGC","Manufacturer=""Kingbright""",ManufacturerPartNumber=KPT-1608SGC,MARK=,NOM=,PCB3D=,"Pin Info=",Power_Voltage=,"Signal Integrity=",Simulation=,TKE=0603,Tolerance=,Value=,Ïðèìå÷àíèå=|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=EVU-LI-2.0.SCHLIB\RC0402FR-071KL|DESIGNITEMID=RC0402FR-071KL|ITEMSOURCE=EVU-LI-2.0.SCHLIB|STATUS=Unknown|DESCRIPTION=0402 1 kOhm ±1% 0.063W|USERCOMMENTS=RC0402FR-071KL|NOTE=|LINENUMBER=|SELECTEDPARAMETERSHASH="0402 1 kOhm ±1% 0.063W",1K,RC0402FR-071KL|COMPONENTPARAMETERS=Comment=RC0402FR-071KL,"Component Kind=Standard",ComponentHeight=0.35mm,ComponentLink1Description=DataSheet,ComponentLink1URL=\\STORAGE\Lib_PCAD\LIB_DataSheet\RESISTORS\BOURNS\CR_0402.pdf,"Description=0402 1 kOhm ±1% 0.063W",Footprint=RESC1005X35N,"Ibis Model=","Library Name=EVU-LI-2.0.SCHLIB","Library Reference=RC0402FR-071KL","Manufacturer=""Yageo""",ManufacturerPartNumber=RC0402FR-071KL,MARK=102,"NOM=0402 1K ±1% 0,0625 W",PCB3D=,"Pin Info=","Power_Voltage=0,0625 W","Signal Integrity=",Simulation=,TKE=0402,Tolerance=±1%,Value=1K,"Value Ru=1 êÎì",Ïðèìå÷àíèå=|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=EVU-LI-2.1.SCHLIB\RC0402FR-0710KL|DESIGNITEMID=RC0402FR-0710KL|ITEMSOURCE=EVU-LI-2.1.SCHLIB|STATUS=Ambiguous component|DESCRIPTION=0402 10 kOhm ±1% 0.063W|USERCOMMENTS=RC0402FR-0710KL|NOTE=|LINENUMBER=|SELECTEDPARAMETERSHASH="0402 10 kOhm ±1% 0.063W",10K,RC0402FR-0710KL|COMPONENTPARAMETERS=Comment=RC0402FR-0710KL,"Component Kind=Standard",ComponentHeight=0.35mm,ComponentLink1Description=DataSheet,ComponentLink1URL=\\STORAGE\Lib_PCAD\LIB_DataSheet\RESISTORS\BOURNS\CR_0402.pdf,"Description=0402 10 kOhm ±1% 0.063W",DNP=,Footprint=RESC1005X35N,"Ibis Model=","Library Name=EVU-LI-2.1.SCHLIB","Library Reference=RC0402FR-0710KL","Manufacturer=""Yageo""",ManufacturerPartNumber=RC0402FR-0710KL,MARK=103,"NOM=0402 10K ±1% 0,0625 W",PCB3D=,"Pin Info=","Power_Voltage=0,0625 W","Signal Integrity=",Simulation=,TKE=0402,Tolerance=±1%,Value=10K,"Value Ru=10 êÎì",Ïðèìå÷àíèå=|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=EVU-LI-2.0.SCHLIB\RC0402FR-07100KL|DESIGNITEMID=RC0402FR-07100KL|ITEMSOURCE=EVU-LI-2.0.SCHLIB|STATUS=Unknown|DESCRIPTION=0402 100 kOhm ±1% 0.063W|USERCOMMENTS=RC0402FR-07100KL|NOTE=|LINENUMBER=|SELECTEDPARAMETERSHASH="0402 100 kOhm ±1% 0.063W",100K,RC0402FR-07100KL|COMPONENTPARAMETERS=Comment=RC0402FR-07100KL,"Component Kind=Standard",ComponentHeight=0.35mm,ComponentLink1Description=DataSheet,ComponentLink1URL=\\STORAGE\Lib_PCAD\LIB_DataSheet\RESISTORS\BOURNS\CR_0402.pdf,"Description=0402 100 kOhm ±1% 0.063W",Footprint=RESC1005X35N,"Ibis Model=","Library Name=EVU-LI-2.0.SCHLIB","Library Reference=RC0402FR-07100KL","Manufacturer=""Yageo""",ManufacturerPartNumber=RC0402FR-07100KL,MARK=103,"NOM=0402 100K ±1% 0,0625 W",PCB3D=,"Pin Info=","Power_Voltage=0,0625 W","Signal Integrity=",Simulation=,TKE=0402,Tolerance=±1%,Value=100K,"Value Ru=100 êÎì",Ïðèìå÷àíèå=|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=EVU-LI-2.0.SCHLIB\CR0402-JW-202-G|DESIGNITEMID=CR0402-JW-202-G|ITEMSOURCE=EVU-LI-2.0.SCHLIB|STATUS=Unknown|DESCRIPTION=0402 2 kOhm±5% 0.063W|USERCOMMENTS=CR0402-JW-202-G|NOTE=|LINENUMBER=|SELECTEDPARAMETERSHASH="0402 2 kOhm±5% 0.063W",2K,CR0402-JW-202-G|COMPONENTPARAMETERS=Comment=CR0402-JW-202-G,"Component Kind=Standard",ComponentHeight=0.35mm,ComponentLink1Description=DataSheet,ComponentLink1URL=\\STORAGE\Lib_PCAD\LIB_DataSheet\RESISTORS\BOURNS\CR_0402.pdf,"Description=0402 2 kOhm±5% 0.063W",Footprint=RESC1005X35N,"Ibis Model=","Library Name=EVU-LI-2.0.SCHLIB","Library Reference=CR0402-JW-202-G","Manufacturer=""Bourns""",ManufacturerPartNumber=CR0402-JW-202-G,MARK=202,"NOM=0402 2K ±5% 0,0625 W",PCB3D=,"Pin Info=","Power_Voltage=0,0625 W","Signal Integrity=",Simulation=,TKE=0402,Tolerance=±5%,Value=2K,"Value Ru=2 êÎì",Ïðèìå÷àíèå=|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=EVU-LI-2.0.SCHLIB\CR0402-JW-331-G|DESIGNITEMID=CR0402-JW-331-G|ITEMSOURCE=EVU-LI-2.0.SCHLIB|STATUS=Unknown|DESCRIPTION=0402 330 Ohm±5% 0.063W|USERCOMMENTS=CR0402-JW-331-G|NOTE=|LINENUMBER=|SELECTEDPARAMETERSHASH="0402 330 Ohm±5% 0.063W",330R,CR0402-JW-331-G|COMPONENTPARAMETERS=Comment=CR0402-JW-331-G,"Component Kind=Standard",ComponentHeight=0.35mm,ComponentLink1Description=DataSheet,ComponentLink1URL=\\STORAGE\Lib_PCAD\LIB_DataSheet\RESISTORS\BOURNS\CR_0402.pdf,"Description=0402 330 Ohm±5% 0.063W",DNP=,Footprint=RESC1005X35N,"Ibis Model=","Library Name=EVU-LI-2.0.SCHLIB","Library Reference=CR0402-JW-331-G","Manufacturer=""Bourns""",ManufacturerPartNumber=CR0402-JW-331-G,MARK=331,"NOM=0402 330R ±5% 0,0625 W",PCB3D=,"Pin Info=","Power_Voltage=0,0625 W","Signal Integrity=",Simulation=,TKE=0402,Tolerance=±5%,Value=330R,"Value Ru=330 Îì",Ïðèìå÷àíèå=|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=EVU-LI-2.0.SCHLIB\RC0402FR-070RL|DESIGNITEMID=RC0402FR-070RL|ITEMSOURCE=EVU-LI-2.0.SCHLIB|STATUS=Unknown|DESCRIPTION=0402 0 Ohm ±1% 0.063W|USERCOMMENTS=RC0402FR-070RL|NOTE=|LINENUMBER=|SELECTEDPARAMETERSHASH="0402 0 Ohm ±1% 0.063W",0R,RC0402FR-070RL|COMPONENTPARAMETERS=Comment=RC0402FR-070RL,"Component Kind=Standard",ComponentHeight=0.35mm,ComponentLink1Description=DataSheet,ComponentLink1URL=\\STORAGE\Lib_PCAD\LIB_DataSheet\RESISTORS\BOURNS\CR_0402.pdf,"Description=0402 0 Ohm ±1% 0.063W",Footprint=RESC1005X35N,"Ibis Model=","Library Name=EVU-LI-2.0.SCHLIB","Library Reference=RC0402FR-070RL","Manufacturer=""Yageo""",ManufacturerPartNumber=RC0402FR-070RL,MARK=000,"NOM=0402 0R ±1% 0,0625 W",PCB3D=,"Pin Info=","Power_Voltage=0,0625 W","Signal Integrity=",Simulation=,TKE=0402,Tolerance=±1%,Value=0R,"Value Ru=0 Îì",Ïðèìå÷àíèå=|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=EVU-LI-2.0.SCHLIB\RC0402FR-0791RL|DESIGNITEMID=RC0402FR-0791RL|ITEMSOURCE=EVU-LI-2.0.SCHLIB|STATUS=Unknown|DESCRIPTION=0402 91 Ohm ±1% 0.063W|USERCOMMENTS=RC0402FR-0791RL|NOTE=|LINENUMBER=|SELECTEDPARAMETERSHASH="0402 91 Ohm ±1% 0.063W",91R,RC0402FR-0791RL|COMPONENTPARAMETERS=Comment=RC0402FR-0791RL,"Component Kind=Standard",ComponentHeight=0.35mm,ComponentLink1Description=DataSheet,ComponentLink1URL=\\STORAGE\Lib_PCAD\LIB_DataSheet\RESISTORS\BOURNS\CR_0402.pdf,"Description=0402 91 Ohm ±1% 0.063W",Footprint=RESC1005X35N,"Ibis Model=","Library Name=EVU-LI-2.0.SCHLIB","Library Reference=RC0402FR-0791RL","Manufacturer=""Yageo""",ManufacturerPartNumber=RC0402FR-0791RL,MARK=102,"NOM=0402 91R ±1% 0,0625 W",PCB3D=,"Pin Info=","Power_Voltage=0,0625 W","Signal Integrity=",Simulation=,TKE=0402,Tolerance=±1%,Value=91R,"Value Ru=91 Îì",Ïðèìå÷àíèå=|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=EVU-LI-2.0.SCHLIB\RC0402FR-07130RL|DESIGNITEMID=RC0402FR-07130RL|ITEMSOURCE=EVU-LI-2.0.SCHLIB|STATUS=Unknown|DESCRIPTION=0402 130 Ohm ±1% 0.063W|USERCOMMENTS=RC0402FR-07130RL|NOTE=|LINENUMBER=|SELECTEDPARAMETERSHASH="0402 130 Ohm ±1% 0.063W",130R,RC0402FR-07130RL|COMPONENTPARAMETERS=Comment=RC0402FR-07130RL,"Component Kind=Standard",ComponentHeight=0.35mm,ComponentLink1Description=DataSheet,ComponentLink1URL=\\STORAGE\Lib_PCAD\LIB_DataSheet\RESISTORS\BOURNS\CR_0402.pdf,"Description=0402 130 Ohm ±1% 0.063W",Footprint=RESC1005X35N,"Ibis Model=","Library Name=EVU-LI-2.0.SCHLIB","Library Reference=RC0402FR-07130RL","Manufacturer=""Yageo""",ManufacturerPartNumber=RC0402FR-07130RL,MARK=102,"NOM=0402 130R ±1% 0,0625 W",PCB3D=,"Pin Info=","Power_Voltage=0,0625 W","Signal Integrity=",Simulation=,TKE=0402,Tolerance=±1%,Value=130R,"Value Ru=130 Îì",Ïðèìå÷àíèå=|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=EVU-LI-2.1.SCHLIB\RC0402FR-071KL|DESIGNITEMID=RC0402FR-071KL|ITEMSOURCE=EVU-LI-2.1.SCHLIB|STATUS=Unknown|DESCRIPTION=0402 1 kOhm ±1% 0.063W|USERCOMMENTS=RC0402FR-071KL|NOTE=|LINENUMBER=|SELECTEDPARAMETERSHASH="0402 1 kOhm ±1% 0.063W",1K,RC0402FR-071KL|COMPONENTPARAMETERS=Comment=RC0402FR-071KL,"Component Kind=Standard",ComponentHeight=0.35mm,ComponentLink1Description=DataSheet,ComponentLink1URL=\\STORAGE\Lib_PCAD\LIB_DataSheet\RESISTORS\BOURNS\CR_0402.pdf,"Description=0402 1 kOhm ±1% 0.063W",Footprint=RESC1005X35N,"Ibis Model=","Library Name=EVU-LI-2.1.SCHLIB","Library Reference=RC0402FR-071KL","Manufacturer=""Yageo""",ManufacturerPartNumber=RC0402FR-071KL,MARK=102,"NOM=0402 1K ±1% 0,0625 W",PCB3D=,"Pin Info=","Power_Voltage=0,0625 W","Signal Integrity=",Simulation=,TKE=0402,Tolerance=±1%,Value=1K,"Value Ru=1 êÎì",Ïðèìå÷àíèå=|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=EVU-LI-2.1.SCHLIB\RC0402FR-07100KL|DESIGNITEMID=RC0402FR-07100KL|ITEMSOURCE=EVU-LI-2.1.SCHLIB|STATUS=Unknown|DESCRIPTION=0402 100 kOhm ±1% 0.063W|USERCOMMENTS=RC0402FR-07100KL|NOTE=|LINENUMBER=|SELECTEDPARAMETERSHASH="0402 100 kOhm ±1% 0.063W",100K,RC0402FR-07100KL|COMPONENTPARAMETERS=Comment=RC0402FR-07100KL,"Component Kind=Standard",ComponentHeight=0.35mm,ComponentLink1Description=DataSheet,ComponentLink1URL=\\STORAGE\Lib_PCAD\LIB_DataSheet\RESISTORS\BOURNS\CR_0402.pdf,"Description=0402 100 kOhm ±1% 0.063W",DNP=,Footprint=RESC1005X35N,"Ibis Model=","Library Name=EVU-LI-2.1.SCHLIB","Library Reference=RC0402FR-07100KL","Manufacturer=""Yageo""",ManufacturerPartNumber=RC0402FR-07100KL,MARK=103,"NOM=0402 100K ±1% 0,0625 W",PCB3D=,"Pin Info=","Power_Voltage=0,0625 W","Signal Integrity=",Simulation=,TKE=0402,Tolerance=±1%,Value=100K,"Value Ru=100 êÎì",Ïðèìå÷àíèå=|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=EVU-LI-2.0.SCHLIB\DHN-02-V-T/R|DESIGNITEMID=DHN-02-V-T/R|ITEMSOURCE=EVU-LI-2.0.SCHLIB|STATUS=Unknown|DESCRIPTION=2 switches in case|USERCOMMENTS=DHN-02-V-T/R|NOTE=|LINENUMBER=|SELECTEDPARAMETERSHASH="2 switches in case",DHN-02-V-T/R|COMPONENTPARAMETERS=Comment=DHN-02-V-T/R,"Component Kind=Standard","Description=2 switches in case",ENGname=,"ESKDname=Ïåðåêëþ÷àòåëü DHN-02-V-T/R",Footprint=A6H-21,"Height=1.6 mm","Ibis Model=","Library Name=EVU-LI-2.0.SCHLIB","Library Reference=DHN-02-V-T/R","Manufacturer=""DIPTRONICS""",Note=,PartNumber=DHN-02-V-T/R,PCB3D=,"Pin Info=","Signal Integrity=",Simulation=,Type=Ïåðåêëþ÷àòåëü|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=EVU-LI-2.0.SCHLIB\KLS7-TS3606-3.5-180|DESIGNITEMID=KLS7-TS3606-3.5-180|ITEMSOURCE=EVU-LI-2.0.SCHLIB|STATUS=Unknown|DESCRIPTION=Kind of Tactile Switch|USERCOMMENTS=KLS7-TS3606-3.5-180|NOTE=|LINENUMBER=|SELECTEDPARAMETERSHASH="Kind of Tactile Switch",KLS7-TS3606-3.5-180|COMPONENTPARAMETERS=Comment=KLS7-TS3606-3.5-180,"Component Kind=Standard","Description=Kind of Tactile Switch",ENGname=,"ESKDname=Êíîïêà òàêòîâàÿ KLS7-TS3606-3.5-180",Footprint=KLS7-TS3606-3.5-180,"Ibis Model=","Library Name=EVU-LI-2.0.SCHLIB","Library Reference=KLS7-TS3606-3.5-180","Manufacturer=""KLS""",Note=,PartNumber=KLS7-TS3606-3.5-180,PCB3D=,"Pin Info=","Signal Integrity=",Simulation=,"Type=Êíîïêà òàêòîâàÿ"|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=EVU-LI-2.0.SCHLIB\1N5817W|DESIGNITEMID=1N5817W|ITEMSOURCE=EVU-LI-2.0.SCHLIB|STATUS=Unknown|DESCRIPTION=Diode Schottky 20V 1A [SOD-123]|USERCOMMENTS=1N5817W|NOTE=|LINENUMBER=|SELECTEDPARAMETERSHASH=1N5817W,"Diode Schottky 20V 1A [SOD-123]"|COMPONENTPARAMETERS=Comment=1N5817W,"Component Kind=Standard","Description=Diode Schottky 20V 1A [SOD-123]",ENGname=,"ESKDname=* 1N5817W, *",Footprint=DIOD_SOD-123,"Ibis Model=","Library Name=EVU-LI-2.0.SCHLIB","Library Reference=1N5817W","Manufacturer=HOTTECH ELECTRONICS",Note=,Package=,PartNumber=1N5817W,PCB3D=,"Pin Info=","Signal Integrity=",Simulation=,Type=|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=EVU-LI-2.1.SCHLIB\BSS8402DW-7-F|DESIGNITEMID=BSS8402DW-7-F|ITEMSOURCE=EVU-LI-2.1.SCHLIB|STATUS=Unknown|DESCRIPTION=MOSFET N/P-CH 60V/50V SC70-6|USERCOMMENTS=BSS8402DW-7-F|NOTE=|LINENUMBER=|SELECTEDPARAMETERSHASH=BSS8402DW-7-F,"MOSFET N/P-CH 60V/50V SC70-6"|COMPONENTPARAMETERS=Automotive=No,"Automotive Grade=NA",Category=Trans,Comment=BSS8402DW-7-F,"Component Kind=Standard",ComponentLink2Description=Datasheet,ComponentLink2URL=https://www.diodes.com/assets/Datasheets/ds30380.pdf,"Continuous Drain Current=115/-130mA","Depletion Mode=False","Description=MOSFET N/P-CH 60V/50V SC70-6","Device Class L1=Discrete Semiconductors","Device Class L2=Transistors","Device Class L3=MOSFETs","Digikey Description=MOSFET N/P-CH 60V/50V SC70-6","Drain To Source Breakdown Voltage=70/-50V","Drain To Source Resistance=4.4/10?","Drain To Source Voltage=60/-50V",Footprint=FP-SOT363-MFG,"Footprint Url=https://www.diodes.com/assets/Package-Files/SOT363.pdf","Gate To Source Voltage=20V",Height=1.1mm,"Ibis Model=","Lead Free=Yes","Library Name=EVU-LI-2.1.SCHLIB","Library Reference=BSS8402DW-7-F",Manufacturer=Diodes,"Manufacturer Part Number=BSS8402DW-7-F","Max Junction Temp=+150°C","Mouser Description=MOSFET 60 / -50V 200mW","Number Of Channels=2","Number Of N Channels=1","Number Of P Channels=1",Octopart=https://octopart.com/bss8402dw-7-f-diodes+inc.-335912,Package=SOT363,PCB3D=,"Pin Info=","Power Dissipation=200mW","Pulse Drain Current=800mA",RoHS=TRUE,"Rthja Max=625°C/W","Signal Integrity=",Simulation=,"Standoff Height=0mm","Temperature=-55°C to +150°C","Temperature Range High=+150°C","Temperature Range Low=-55°C","Threshold Vgs Max=2.5/-2V","Threshold Vgs Min=1/-0.8V",Transconductance=0.08/0.05S,"Turn Off Delay Time=11/18ns","Turn On Delay Time=7/10ns"|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=EVU-LI-2.0.SCHLIB\DS1021-1x12|DESIGNITEMID=DS1021-1x12|ITEMSOURCE=EVU-LI-2.0.SCHLIB|STATUS=Unknown|DESCRIPTION=Connector 2.54 pitch, 1 rows, 8.54 height|USERCOMMENTS=DS1021-1x12|NOTE=|LINENUMBER=|SELECTEDPARAMETERSHASH=,"Connector 2.54 pitch, 1 rows, 8.54 height",DS1021-1x12|COMPONENTPARAMETERS=Comment=DS1021-1x12,"Component Kind=Standard",ComponentHeight=8.54mm,ComponentLink1Description=DataSheet,"ComponentLink1URL=\\STORAGE\Lib_PCAD\LIB_DataSheet\CONNECTORS\ÒÄ Áóðûé ìåäâåäü\PLS_BLS.pdf","Description=Connector 2.54 pitch, 1 rows, 8.54 height",Footprint=PLS-12,"Ibis Model=","Library Name=EVU-LI-2.0.SCHLIB","Library Reference=DS1021-1x12","Manufacturer=""Connfly""","ManufacturerPartNumber=DS1021-1x12 (PLS-12)",MARK=,NOM=,PCB3D=,"Pin Info=",Power_Voltage=,"Signal Integrity=",Simulation=,TKE=,Tolerance=,Value=,Ïðèìå÷àíèå=|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=EVU-LI-2.0.SCHLIB\TYPE-C-31-M-12|DESIGNITEMID=TYPE-C-31-M-12|ITEMSOURCE=EVU-LI-2.0.SCHLIB|STATUS=Unknown|DESCRIPTION=USB TYPE-C 5A 16P Female SMD USB Connectors|USERCOMMENTS=TYPE-C-31-M-12|NOTE=|LINENUMBER=|SELECTEDPARAMETERSHASH=,TYPE-C-31-M-12,"USB TYPE-C 5A 16P Female SMD USB Connectors"|COMPONENTPARAMETERS="Availability=In Stock",Check_prices=https://www.snapeda.com/parts/USB4800-03-A/Global+Connector+Technology/view-part/?ref=eda,Comment=TYPE-C-31-M-12,"Component Kind=Standard","Description=USB TYPE-C 5A 16P Female SMD USB Connectors",Footprint=TYPE-C-31-M-12,"Ibis Model=","Library Name=EVU-LI-2.0.SCHLIB","Library Reference=TYPE-C-31-M-12","Manufacturer=""GCT""",ManufacturerPartNumber=USB4800-03-A,"MF=Global Connector Technology",MP=USB4800-03-A,Package=None,PCB3D=,"Pin Info=",Price=None,Purchase-URL=https://pricing.snapeda.com/search/part/USB4800-03-A/?ref=eda,"Signal Integrity=",Simulation=,SnapEDA_Link=https://www.snapeda.com/parts/USB4800-03-A/Global+Connector+Technology/view-part/?ref=snap,Value=|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=EVU-LI-2.1.SCHLIB\GRM21BR61C106KE15L|DESIGNITEMID=GRM21BR61C106KE15L|ITEMSOURCE=EVU-LI-2.1.SCHLIB|STATUS=Unknown|DESCRIPTION=0805 X5R 10uF±10% 16V|USERCOMMENTS=GRM21BR61C106KE15L|NOTE=|LINENUMBER=|SELECTEDPARAMETERSHASH="0805 X5R 10uF±10% 16V",10uF,GRM21BR61C106KE15L|COMPONENTPARAMETERS=Comment=GRM21BR61C106KE15L,"Component Kind=Standard",ComponentHeight=1.3mm,ComponentLink1Description=DataSheet,"ComponentLink1URL=\\STORAGE\Lib_PCAD\LIB_DataSheet\Capacitors\Murata Chip Monolithic Ceramic Capacitors.pdf","Description=0805 X5R 10uF±10% 16V",Footprint=CAPC2012X125N,"Ibis Model=","Library Name=EVU-LI-2.1.SCHLIB","Library Reference=GRM21BR61C106KE15L","Manufacturer=""Murata""",ManufacturerPartNumber=GRM21BR61C106KE15L,"NOM=0805 X5R 10uF ±10% 16V",PCB3D=,"Pin Info=",Power_Voltage=16V,"Signal Integrity=",Simulation=,"TKE=0805 X5R",Tolerance=±10%,Value=10uF,"Value Ru=10 ìêÔ",Ïðèìå÷àíèå=|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=EVU-LI-2.1.SCHLIB\DMG1012T-7|DESIGNITEMID=DMG1012T-7|ITEMSOURCE=EVU-LI-2.1.SCHLIB|STATUS=Unknown|DESCRIPTION=N-Channel Enhancement Mode MOSFET, 20 V, 630 mA, -55 to 150 degC, 3-Pin SOT23, RoHS, Tape and Reel|USERCOMMENTS=DMG1012T-7|NOTE=|LINENUMBER=|SELECTEDPARAMETERSHASH=DMG1012T-7,"N-Channel Enhancement Mode MOSFET, 20 V, 630 mA, -55 to 150 degC, 3-Pin SOT23, RoHS, Tape and Reel"|COMPONENTPARAMETERS=Case\/Package=SOT-523,Comment=DMG1012T-7,"Component Kind=Standard","Contact Plating=Matte","Continuous Drain Current (ID)=630mA","Datasheet URL=https://www.diodes.com/assets/Datasheets/ds31783.pdf","Datasheet Version=Rev. 3-2, 01/2012","Description=N-Channel Enhancement Mode MOSFET, 20 V, 630 mA, -55 to 150 degC, 3-Pin SOT23, RoHS, Tape and Reel","Drain to Source Breakdown Voltage=20V","Drain to Source Resistance=300mOhm","Drain to Source Voltage (Vdss)=20V","Element Configuration=Single","Fall Time=12.3ns",Footprint=DIOD-SOT523-3_V,"Gate to Source Voltage (Vgs)=6V",Height=0.8mm,"Ibis Model=","Input Capacitance=60.67pF","Lead Free=LeadFree",Length=1.7mm,"Library Name=EVU-LI-2.1.SCHLIB","Library Reference=DMG1012T-7","Manufacturer=Diodes Inc","Manufacturer URL=http://www.diodes.com/","Max Operating Temperature=150degC","Max Power Dissipation=280mW","Min Operating Temperature=-55degC",Mount=SurfaceMount,"Mounting Technology=SurfaceMount","Number of Channels=1","Number of Elements=1","Number of Pins=3","On-State Resistance=400MOhm","Package Description=3-Pin Small Outline Transistor, Body 1.6 x 0.8 mm, Pitch 0.5 mm","Package Quantity=3000","Package Reference=SOT523-3",Packaging=TapeandReel,PCB3D=,"Pin Info=","Power Dissipation=280mW","Radiation Hardening=No","Rds On Max=400mOhm","REACH SVHC=NoSVHC","Rise Time=7.4ns",RoHSCompliant=true,"Signal Integrity=",Simulation=,"Threshold Voltage=1V","Turn-Off Delay Time=26.7ns","Turn-On Delay Time=5.1ns",Weight=7.1E-05oz,Width=0.85mm|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
